(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 60)
    (tracks 757)
    (zones 0)
    (modules 66)
    (nets 60)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.7)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8 0.5)
    (user_via 0.9 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 0.8 0.8)
    (mod_edge_width 0.1)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.1)
    (pad_size 2.08 3.6)
    (pad_drill 1.4)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 100 100)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GNDA)
  (net 2 "Net-(AE1-Pad1)")
  (net 3 +3V3)
  (net 4 VCC)
  (net 5 /RWD)
  (net 6 "Net-(C5-Pad1)")
  (net 7 +4V)
  (net 8 /SIM_RST)
  (net 9 /SIM_VDD)
  (net 10 /SIM_DAT)
  (net 11 /SIM_CLK)
  (net 12 "Net-(D1-Pad2)")
  (net 13 /RST)
  (net 14 /485_A)
  (net 15 /485_B)
  (net 16 /CLK)
  (net 17 /MOSI)
  (net 18 /LED)
  (net 19 /DC)
  (net 20 /CS)
  (net 21 /HS_TXD)
  (net 22 /HS_RXD)
  (net 23 /U1_RXD)
  (net 24 /U1_TXD)
  (net 25 /WDI)
  (net 26 "Net-(R3-Pad2)")
  (net 27 "Net-(R4-Pad2)")
  (net 28 /U2_TXD)
  (net 29 "Net-(R13-Pad2)")
  (net 30 /U2_RXD)
  (net 31 "Net-(R14-Pad2)")
  (net 32 "Net-(R15-Pad2)")
  (net 33 /I2C_SDA)
  (net 34 /I2C_SCL)
  (net 35 "Net-(D2-Pad1)")
  (net 36 "Net-(D5-Pad2)")
  (net 37 /RES)
  (net 38 "Net-(R6-Pad1)")
  (net 39 "Net-(R11-Pad2)")
  (net 40 "Net-(R12-Pad2)")
  (net 41 "Net-(R16-Pad1)")
  (net 42 "Net-(R17-Pad1)")
  (net 43 "Net-(R5-Pad1)")
  (net 44 "Net-(R8-Pad1)")
  (net 45 /SW)
  (net 46 "Net-(U1-Pad3)")
  (net 47 "Net-(U1-Pad7)")
  (net 48 "Net-(U8-Pad3)")
  (net 49 "Net-(U8-Pad4)")
  (net 50 "Net-(J6-Pad6)")
  (net 51 "Net-(U2-Pad16)")
  (net 52 "Net-(U2-Pad17)")
  (net 53 "Net-(U2-Pad18)")
  (net 54 "Net-(U2-Pad19)")
  (net 55 "Net-(U2-Pad24)")
  (net 56 "Net-(Q1-Pad3)")
  (net 57 /BL)
  (net 58 "Net-(U2-Pad12)")
  (net 59 "Net-(U2-Pad14)")
  (net_class Default 这是默认网络组.
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.7)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +4V)
    (add_net /485_A)
    (add_net /485_B)
    (add_net /BL)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DC)
    (add_net /HS_RXD)
    (add_net /HS_TXD)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /LED)
    (add_net /MOSI)
    (add_net /RES)
    (add_net /RST)
    (add_net /RWD)
    (add_net /SIM_CLK)
    (add_net /SIM_DAT)
    (add_net /SIM_RST)
    (add_net /SIM_VDD)
    (add_net /SW)
    (add_net /U1_RXD)
    (add_net /U1_TXD)
    (add_net /U2_RXD)
    (add_net /U2_TXD)
    (add_net /WDI)
    (add_net GNDA)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U8-Pad3)")
    (add_net "Net-(U8-Pad4)")
    (add_net VCC)
  )
  (module Connector_Phoenix_MC_HighVoltage:PhoenixContact_MC_1,5_4-G-5.08_1x04_P5.08mm_Horizontal (layer F.Cu) (tedit 5A00FA1B)
    (at 103.25 72.38 270)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/4-G-5.08; number of pins: 04; pin pitch: 5.08mm; Angled || order number: 1836202 8A 320V")
    (tags "phoenix_contact connector MC_01x04_G_5.08mm")
    (fp_text reference J1 (at 7.62 -2.8 270) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 7.62 9 270) (layer F.Fab))
    (fp_text user %R (at 7.62 3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 3 thru_hole oval (at 10.16 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 /485_A))
    (pad 4 thru_hole oval (at 15.24 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /485_B))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MC_1,5_4-G-5.08_1x04_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_RF_Modules:Air202 placed (layer F.Cu) (tedit 5B6EDD58)
    (at 137.2 80)
    (attr smd)
    (fp_text reference U2 (at 2.7 1 180) (layer F.SilkS))
    (fp_text value Air202 (at 0 -4.2) (layer F.Fab))
    (pad 1 smd oval (at -6.95 -6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 36 smd rect (at 0 1.5 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 36 smd rect (at 4.2 6 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 36 smd rect (at -4.2 6 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 38 smd oval (at -4.2 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +4V))
    (pad 37 smd oval (at -3 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +4V))
    (pad 36 smd oval (at -1.8 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 35 smd oval (at -0.6 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 34 smd oval (at 0.6 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /RST))
    (pad 33 smd oval (at 1.8 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 32 smd oval (at 3.3 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(AE1-Pad1)") (clearance 0.6))
    (pad 31 smd oval (at 4.8 -8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 12 smd oval (at -4.2 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U2-Pad12)"))
    (pad 13 smd oval (at -3 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /LED))
    (pad 14 smd oval (at -1.8 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U2-Pad14)"))
    (pad 15 smd oval (at -0.6 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 16 smd oval (at 0.6 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad16)"))
    (pad 17 smd oval (at 1.8 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-Pad17)"))
    (pad 18 smd oval (at 3 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad18)"))
    (pad 19 smd oval (at 4.2 8.4) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U2-Pad19)"))
    (pad 30 smd oval (at 6.95 -6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /I2C_SDA))
    (pad 2 smd oval (at -6.95 -4.8 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /CS))
    (pad 29 smd oval (at 6.95 -4.8 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /I2C_SCL))
    (pad 3 smd oval (at -6.95 -3.6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /CLK))
    (pad 28 smd oval (at 6.95 -3.6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R11-Pad2)"))
    (pad 4 smd oval (at -6.95 -2.4 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /MOSI))
    (pad 27 smd oval (at 6.95 -2.4 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R12-Pad2)"))
    (pad 5 smd oval (at -6.95 -1.2 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /DC))
    (pad 26 smd oval (at 6.95 -1.2 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R13-Pad2)"))
    (pad 6 smd oval (at -6.95 0 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 37 /RES))
    (pad 25 smd oval (at 6.95 0 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R14-Pad2)"))
    (pad 7 smd oval (at -6.95 1.2 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 57 /BL))
    (pad 24 smd oval (at 6.95 1.2 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-Pad24)"))
    (pad 8 smd oval (at -6.95 2.4 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R3-Pad2)"))
    (pad 23 smd oval (at 6.95 2.4 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R15-Pad2)"))
    (pad 9 smd oval (at -6.95 3.6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (pad 22 smd oval (at 6.95 3.6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R16-Pad1)"))
    (pad 10 smd oval (at -6.95 4.8 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /WDI))
    (pad 21 smd oval (at 6.95 4.8 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /SIM_VDD))
    (pad 11 smd oval (at -6.95 6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /RWD))
    (pad 20 smd oval (at 6.95 6 90) (size 0.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R17-Pad1)"))
  )
  (module My_LED:LED-3-6.4-7.5mm (layer F.Cu) (tedit 5BA4A364)
    (at 100.1 93.1 90)
    (fp_text reference D5 (at 0 0.8 90) (layer F.SilkS))
    (fp_text value RED (at -3.2 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 4.3 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole rect (at 1.27 4.3 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm.wrl
      (offset (xyz 1.5 -4.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 155.6 70.98)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /U2_TXD))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /U2_RXD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical (layer F.Cu) (tedit 5A0E414C)
    (at 127.5 74 270)
    (descr "JST PH series connector, B8B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference J2 (at 7 -2.9 270) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 7 4 270) (layer F.Fab))
    (fp_text user %R (at 7 1.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 /CLK))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 /MOSI))
    (pad 5 thru_hole oval (at 8 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 37 /RES))
    (pad 6 thru_hole oval (at 10 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 /DC))
    (pad 7 thru_hole oval (at 12 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 /CS))
    (pad 8 thru_hole oval (at 14 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 57 /BL))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 119.9 79.9 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 5551 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /U1_TXD))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_6.3x7.7 locked (layer F.Cu) (tedit 5A841F9D)
    (at 111.9 70.4 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7, Nichicon ")
    (tags "Capacitor Electrolytic")
    (clearance 0.5)
    (attr smd)
    (fp_text reference C3 (at 0 -4.35 270) (layer F.SilkS))
    (fp_text value 100uF (at 0 4.35 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 5A841F9D)
    (at 120 71.85 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5, Vishay 0810 http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C6 (at 0 -5.3 270) (layer F.SilkS))
    (fp_text value 1mF (at 0 5.3 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.7 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +4V))
    (pad 2 smd rect (at 3.7 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.6 88.6)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /SIM_CLK))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.9 84.6 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -1.8 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.05 90.2 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.05 0.8 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RWD))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.2 69.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +4V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.75 95.4 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.17 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /SIM_DAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133 69.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +4V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.8 69.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +4V))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.4 69.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +4V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.7 68.3)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.7 84.6 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -2 0 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 153.8 95.4 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.17 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SIM_RST))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.2 95.4 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.17 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /SIM_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.6 69.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +4V))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.25 66.45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (clearance 0.5)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "0.1uF 50v" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.1 63.2 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2 0 270) (layer F.SilkS))
    (fp_text value "0.1uF 50v" (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /SW))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Amphenol_901-144_Vertical (layer F.Cu) (tedit 5B6EDD75)
    (at 140.5 64)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical")
    (fp_text reference AE1 (at 0 -2.2) (layer F.SilkS))
    (fp_text value GSM (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(AE1-Pad1)") (clearance 0.4))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 152 70.98)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /HS_TXD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /HS_RXD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA locked (layer F.Cu) (tedit 586432E5)
    (at 104.1 66.8 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (clearance 0.5)
    (attr smd)
    (fp_text reference D1 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value SS14 (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 117.9 93.1)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SS14 (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 /RST))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 107.9 76.3 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D6 (at 0 -0.05 180) (layer F.SilkS))
    (fp_text value SMF6.0CA (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 /485_A))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 107.1 82.6 270)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D7 (at 0 0 270) (layer F.SilkS))
    (fp_text value SMF6.0CA (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 270) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 /485_B))
    (pad 1 smd rect (at -1.4 0 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 /485_A))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 108.5 87.7)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D8 (at 0 0) (layer F.SilkS))
    (fp_text value SMF6.0CA (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 /485_B))
    (pad 2 smd rect (at 1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Taiyo-Yuden_NR-40xx (layer F.Cu) (tedit 5990349D)
    (at 121.15 63.3)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-40xx, 4.0mmx4.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L1 (at 0 -0.05 90) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0) (size 1.2 3.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /SW))
    (pad 2 smd rect (at 1.4 0) (size 1.2 3.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +4V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_NR-40xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 149.9 97.1 90)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK3 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value M_PAD (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GNDA))
  )
  (module MountingHole:MountingHole_2.5mm_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 109.9 62.9 90)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK1 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value M_PAD (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GNDA))
  )
  (module MountingHole:MountingHole_2.5mm_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 109.9 97.1 90)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK2 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value M_PAD (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GNDA))
  )
  (module MountingHole:MountingHole_2.5mm_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 149.9 62.9 270)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK4 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value M_PAD (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0.3 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GNDA))
  )
  (module My_SIM_Card:nano_sim_card_pull locked (layer F.Cu) (tedit 5B6A92F7)
    (at 153.8 87)
    (attr smd)
    (fp_text reference J6 (at 0.02 -7.62) (layer F.SilkS))
    (fp_text value SIM_Card_AIR (at 0.635 -9.525) (layer F.Fab))
    (pad "" np_thru_hole circle (at -4.34 4.15) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 4.66 -4.15) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 smd rect (at -2.54 -5.98) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /SIM_DAT))
    (pad 3 smd rect (at -2.54 5.98) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /SIM_CLK))
    (pad 6 smd rect (at 0 -5.98) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J6-Pad6)"))
    (pad 2 smd rect (at 0 5.98) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /SIM_RST))
    (pad 5 smd rect (at 2.54 -5.98) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 1 smd rect (at 2.54 5.98) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /SIM_VDD))
    (pad 5 smd rect (at 5.4 0) (size 1 3.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 5 smd rect (at -5.4 0) (size 1 3.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 113.95 80.8 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 -0.1 180) (layer F.SilkS))
    (fp_text value SP3485CN (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /485_B))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /485_A))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q1-Pad3)"))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /U1_RXD))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 117.95 88.4)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value watchdog (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R6-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /RWD))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D2-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /WDI))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 122.8 84.7 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value SC662K (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +4V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 115.5 63.6 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (clearance 0.3)
    (attr smd)
    (fp_text reference U3 (at 0 0) (layer F.SilkS))
    (fp_text value JW5026 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R8-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R5-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 45 /SW))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-553 (layer F.Cu) (tedit 5A02FF57)
    (at 156.95 95.5 90)
    (descr SOT553)
    (tags SOT-553)
    (attr smd)
    (fp_text reference U7 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value ESDA6V8AV5 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /SIM_RST))
    (pad 3 smd rect (at -0.7 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /SIM_CLK))
    (pad 5 smd rect (at 0.7 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /SIM_VDD))
    (pad 2 smd rect (at -0.7 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 4 smd rect (at 0.7 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SIM_DAT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.05 88 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 0.85) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R6-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.1 84.6 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.8 0 90) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /WDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 77.6 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 471 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /U2_RXD))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 78.8 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 471 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /HS_TXD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.4 74.1 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /I2C_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 76.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 471 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /U2_TXD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123 81.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.45 0) (layer F.SilkS))
    (fp_text value 471 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /U1_RXD))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.1 64.75 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.5 -0.15 270) (layer F.SilkS))
    (fp_text value 104 (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123 80.25)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.85 0) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(Q1-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.05 89.1 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -0.9) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RWD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 110.085 91.8 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 1.815 0 180) (layer F.SilkS))
    (fp_text value 102 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /LED))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 108.9 81.685 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 1.35 -0.85 90) (layer F.SilkS))
    (fp_text value 471 (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /485_B))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /485_A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123 78.9)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /U1_TXD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 108.9 78.25 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -1.6 0.75) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /485_A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.7 60.9 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -1.3 0 270) (layer F.SilkS))
    (fp_text value 8202 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R8-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +4V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.1 60.9 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 1.25 0.05 270) (layer F.SilkS))
    (fp_text value 2002 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R8-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 83.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 22R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /SIM_DAT))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 86)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 22R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(R17-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SIM_RST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.4 68.33 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /I2C_SCL))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 82.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 22R (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /SIM_CLK))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.8 80 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 471 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R14-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /HS_RXD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 107.6 85.7)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 1.7 0) (layer F.SilkS))
    (fp_text value 472 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /485_B))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_SOIC:AM2320 locked (layer B.Cu) (tedit 5B4180EE)
    (at 158.5 74.79 270)
    (descr AM2320)
    (tags AM2320)
    (fp_text reference U5 (at -6.19 -0.2) (layer F.SilkS))
    (fp_text value AM2320 (at 0.021384 7.98319 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /I2C_SDA))
    (pad 3 thru_hole oval (at 1.27 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 4 thru_hole oval (at 3.81 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /I2C_SCL))
  )
  (module My_Diodes:DFN1006-2L (layer F.Cu) (tedit 5B59D601)
    (at 126.8 69.2 90)
    (descr DFN1006-2L)
    (tags DFN1006-2L)
    (fp_text reference D3 (at 0 -1.1 90) (layer F.SilkS))
    (fp_text value GESDBL4V5Y1 (at 0 1.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.425 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +4V))
    (pad 2 smd rect (at 0.425 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
  )
  (module My_SMD_Packages:DFN-6-1EP_3x3mm_Pitch1mm (layer F.Cu) (tedit 5B59E7A1)
    (at 147.9 71.1)
    (descr "DFN6 3*3 MM, ")
    (tags "DFN 1mm")
    (attr smd)
    (fp_text reference U8 (at -2.15 0 90) (layer F.SilkS))
    (fp_text value SHT20 (at 0 2.75) (layer F.Fab))
    (pad 1 smd rect (at -1 1.4 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /I2C_SDA))
    (pad 2 smd rect (at 0 1.4 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at 1 1.4 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U8-Pad3)"))
    (pad 4 smd rect (at 1 -1.4 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U8-Pad4)"))
    (pad 5 smd rect (at 0 -1.4 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at -1 -1.4 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /I2C_SCL))
    (pad 7 smd rect (at 0 0 90) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text BL (at 125.4 88) (layer B.SilkS))
  (gr_text AM2320 (at 158.7 66.3 90) (layer B.SilkS))
  (gr_text UART2 (at 155.5 66.7 90) (layer B.SilkS))
  (gr_text HOST (at 152 67 90) (layer B.SilkS))
  (gr_text RXD (at 150.1 76.1 90) (layer B.SilkS))
  (gr_text TXD (at 150.1 73.6 90) (layer B.SilkS))
  (gr_text GND (at 150.1 71 90) (layer B.SilkS))
  (gr_text 3V3 (at 153.8 70.9 90) (layer B.SilkS))
  (gr_text SDA (at 157 73.5 90) (layer B.SilkS))
  (gr_text 3V3 (at 157.1 70.9 90) (layer B.SilkS))
  (gr_text TXD (at 153.8 76.1 90) (layer B.SilkS))
  (gr_text "RXD\n" (at 153.8 78.6 90) (layer B.SilkS))
  (gr_text GND (at 153.8 73.4 90) (layer B.SilkS))
  (gr_text CS (at 125.6 86) (layer B.SilkS))
  (gr_text DC (at 125.6 84) (layer B.SilkS))
  (gr_text RES (at 125.2 82) (layer B.SilkS))
  (gr_text SDA (at 125.2 80.1) (layer B.SilkS))
  (gr_text CLK (at 125.3 78) (layer B.SilkS))
  (gr_text 3V3 (at 125.3 76.1) (layer B.SilkS))
  (gr_text GND (at 125.1 74.1) (layer B.SilkS))
  (dimension 59.8 (width 0.15) (layer F.SilkS)
    (gr_text "59.800 mm" (at 129.9 104.8) (layer F.SilkS))
    (feature1 (pts (xy 159.8 98.9) (xy 159.8 105.6)))
    (feature2 (pts (xy 100 98.9) (xy 100 105.6)))
    (crossbar (pts (xy 100 104) (xy 159.8 104)))
    (arrow1a (pts (xy 159.8 104) (xy 158.673496 104.586421)))
    (arrow1b (pts (xy 159.8 104) (xy 158.673496 103.413579)))
    (arrow2a (pts (xy 100 104) (xy 101.126504 104.586421)))
    (arrow2b (pts (xy 100 104) (xy 101.126504 103.413579)))
  )
  (gr_line (start 137.8 100) (end 158.8 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.8 60) (end 137.8 60) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101 60) (end 122 60) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.8 61.6) (end 136.2 61.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 122 61.6) (end 122 60) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.8 98.4) (end 137.8 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122 100) (end 101 100) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 122 98.4) (end 123.6 98.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 40 (width 0.15) (layer F.SilkS)
    (gr_text "40.000 mm" (at 163.742472 79.973185 270) (layer F.SilkS))
    (feature1 (pts (xy 158.942472 99.973185) (xy 164.542472 99.973185)))
    (feature2 (pts (xy 158.942472 59.973185) (xy 164.542472 59.973185)))
    (crossbar (pts (xy 162.942472 59.973185) (xy 162.942472 99.973185)))
    (arrow1a (pts (xy 162.942472 99.973185) (xy 162.356051 98.846681)))
    (arrow1b (pts (xy 162.942472 99.973185) (xy 163.528893 98.846681)))
    (arrow2a (pts (xy 162.942472 59.973185) (xy 162.356051 61.099689)))
    (arrow2b (pts (xy 162.942472 59.973185) (xy 163.528893 61.099689)))
  )
  (gr_text B (at 106 87.7 90) (layer B.SilkS))
  (gr_text SCL (at 157 78.6 90) (layer B.SilkS))
  (gr_text GND (at 157 76.1 90) (layer B.SilkS))
  (gr_text - (at 106 77.6 90) (layer B.SilkS))
  (gr_text + (at 106.1 72.3) (layer B.SilkS))
  (gr_text A (at 106 82.5 90) (layer B.SilkS))
  (gr_arc (start 129.9 61.6) (end 136.2 61.6) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 129.9 98.4) (end 123.6 98.4) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 61) (end 100 99) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.8 61) (end 159.8 99) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 158.8 99) (end 159.8 99) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 158.8 61) (end 158.8 60) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 101 61) (end 100 61) (angle 89.9) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 101 99) (end 101 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.9 60) (xy 159.9 60) (xy 159.9 100) (xy 99.9 100)
      )
    )
  )
  (zone (net 1) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.9 60) (xy 159.9 60) (xy 159.9 100) (xy 99.9 100)
      )
    )
  )
  (zone (net 7) (net_name +4V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.8 68.9) (xy 124.8 69.4) (xy 125.1 69.7) (xy 134.7 69.7) (xy 134.9 69.9)
        (xy 134.9 71.7) (xy 128.1 71.7) (xy 127.4 71) (xy 121.8 71) (xy 120.3 71)
        (xy 119.6 70.3) (xy 119.619231 70.3) (xy 119.665385 69.1) (xy 119.6 69.1) (xy 119.6 67.8)
        (xy 123.8 67.8) (xy 124.2 68.3)
      )
    )
  )
)
